


2:1 mux using CMOS –




2:1 mux using CMOS Waveform –




TG (Transmission Gate) –



TG (Transmission Gate) -



2:1 mux using TG –



2:1 mux using TG -

